description[de] = <b>EAGLE Design Rules</b>\n<p>\nDie Standard-LPT-Design-Rules sind so gewählt, dass sie für \ndie meisten Anwendungen passen. Sollte ihre Platine \nbesondere Anforderungen haben, treffen Sie die erforderlichen\nEinstellungen hier und speichern die Design Rules unter \neinem neuen Namen ab.<br>\nZwei Lagen 18µm+DK-Cu, durchkontaktiert, Abstand/Struktur = 12mil/12mil.
description[en] = <b>EAGLE Design Rules</b>\n<p>\nThe default Design Rules have been set to cover\na wide range of applications. Your particular design\nmay have different requirements, so please make the\nnecessary adjustments and save your customized\ndesign rules under a new name.
layerSetup = (1*16)
mtCopper = 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm
mtIsolate = 1.5mm 0.15mm 0.2mm 0.15mm 0.2mm 0.15mm 0.2mm 0.15mm 0.2mm 0.15mm 0.2mm 0.15mm 0.2mm 0.15mm 0.2mm
mdWireWire = 12mil
mdWirePad = 12mil
mdWireVia = 12mil
mdPadPad = 12mil
mdPadVia = 12mil
mdViaVia = 12mil
mdSmdPad = 0mil
mdSmdVia = 0mil
mdSmdSmd = 0mil
mdViaViaSameLayer = 8mil
mnLayersViaInSmd = 2
mdCopperDimension = 20mil
mdDrill = 8mil
mdSmdStop = 0mil
msWidth = 12mil
msDrill = 16mil
msMicroVia = 9.99mm
msBlindViaRatio = 0.500000
rvPadTop = 0.250000
rvPadInner = 0.250000
rvPadBottom = 0.250000
rvViaOuter = 0.250000
rvViaInner = 0.250000
rvMicroViaOuter = 0.250000
rvMicroViaInner = 0.250000
rlMinPadTop = 12mil
rlMaxPadTop = 20mil
rlMinPadInner = 12mil
rlMaxPadInner = 20mil
rlMinPadBottom = 12mil
rlMaxPadBottom = 20mil
rlMinViaOuter = 12mil
rlMaxViaOuter = 20mil
rlMinViaInner = 12mil
rlMaxViaInner = 20mil
rlMinMicroViaOuter = 4mil
rlMaxMicroViaOuter = 20mil
rlMinMicroViaInner = 4mil
rlMaxMicroViaInner = 20mil
psTop = -1
psBottom = -1
psFirst = -1
psElongationLong = 100
psElongationOffset = 100
mvStopFrame = 1.000000
mvCreamFrame = 0.000000
mlMinStopFrame = 4mil
mlMaxStopFrame = 4mil
mlMinCreamFrame = 0mil
mlMaxCreamFrame = 0mil
mlViaStopLimit = 0mil
srRoundness = 0.000000
srMinRoundness = 0mil
srMaxRoundness = 0mil
slThermalIsolate = 10mil
slThermalsForVias = 0
dpMaxLengthDifference = 10mm
dpGapFactor = 2.500000
checkGrid = 1
checkAngle = 1
checkFont = 1
checkRestrict = 1
useDiameter = 13
maxErrors = 50
